IPFIX-SELECTOR-MIB DEFINITIONS ::= BEGIN


   IMPORTS
       MODULE-IDENTITY, OBJECT-TYPE, mib-2
           FROM SNMPv2-SMI                              -- [RFC2578]
       TruthValue
           FROM SNMPv2-TC                               -- [RFC2579]
       MODULE-COMPLIANCE, OBJECT-GROUP
           FROM SNMPv2-CONF;                            -- [RFC2580]

   ipfixSelectorMIB MODULE-IDENTITY
       LAST-UPDATED "201206110000Z"         -- 11 June 2012
       ORGANIZATION "IETF IPFIX Working Group"
       CONTACT-INFO
           "WG charter:
             http://www.ietf.org/html.charters/ipfix-charter.html

           Mailing Lists:
             General Discussion: ipfix@ietf.org
             To Subscribe: http://www1.ietf.org/mailman/listinfo/ipfix
             Archive:
         http://www1.ietf.org/mail-archive/web/ipfix/current/index.html

           Editor:
             Thomas Dietz
             NEC Europe Ltd.
             NEC Laboratories Europe
             Network Research Division
             Kurfuersten-Anlage 36
             Heidelberg  69115
             Germany
             Phone: +49 6221 4342-128
             Email: Thomas.Dietz@neclab.eu

             Atsushi Kobayashi
             NTT Information Sharing Platform Laboratories
             3-9-11 Midori-cho
             Musashino-shi, Tokyo  180-8585
             Japan
             Phone: +81-422-59-3978
             Email: akoba@nttv6.net

             Benoit Claise
             Cisco Systems, Inc.
             De Kleetlaan 6a b1
             Diegem  1831





             Belgium
             Phone:  +32 2 704 5622
             Email: bclaise@cisco.com

             Gerhard Muenz
             Technische Universitaet Muenchen
             Department of Informatics
             Chair for Network Architectures and Services (I8)
             Boltzmannstr. 3
             Garching  85748
             Germany
             Email: muenz@net.in.tum.de"

       DESCRIPTION
           "The IPFIX SELECTOR MIB module defined in this section
           provides the standard Filtering and Sampling functions that
           can be referenced in the ipfixSelectionProcessTable.  All
           standard Filtering and Sampling functions MUST be registered
           in the subtree under object ipfixSelectorFunctions
           (1.3.6.1.2.1.194.1.1).  The top-level OIDs in the subtree
           under object ipfixSelectorFunctions MUST be registered in a
           sub-registry maintained by IANA at
           <http://www.iana.org/assignments/smi-numbers/>.

           New Selector Functions MUST be registered at IANA and are
           subject to Expert Review [RFC5226], i.e., review by one of a
           group of experts designated by an IETF Area Director.  The
           group of experts MUST check the requested MIB objects for
           completeness and accuracy of the description.  Requests for
           MIB objects that duplicate the functionality of existing
           objects SHOULD be declined.  The smallest available OID
           SHOULD be assigned to new MIB objects.  The specification
           of new MIB objects SHOULD follow the structure specified in
           [RFC6615] and MUST be published using a well-
           established and persistent publication medium.  The experts
           will initially be drawn from the Working Group Chairs and
           document editors of the IPFIX and PSAMP Working Groups.

           Copyright (c) 2012 IETF Trust and the persons identified as
           authors of the code.  All rights reserved.

           Redistribution and use in source and binary forms, with or
           without modification, is permitted pursuant to, and subject
           to the license terms contained in, the Simplified BSD
           License set forth in Section 4.c of the IETF Trust's
           Legal Provisions Relating to IETF Documents
           (http://trustee.ietf.org/license-info)."






   --  Revision history

       REVISION     "201206110000Z"         -- 11 June 2012
       DESCRIPTION
           "Update to MIB description to reflect updated registration
           of new Sampling and Filtering functions.  Published as
           RFC 6615."

       REVISION     "201003150000Z"         -- 15 March 2010
       DESCRIPTION
           "Initial version, published as RFC 5815."

       ::= { mib-2 194 }

   --******************************************************************
   -- Top-Level Structure of the MIB
   --******************************************************************

   ipfixSelectorObjects     OBJECT IDENTIFIER
       ::= { ipfixSelectorMIB 1 }
   ipfixSelectorConformance OBJECT IDENTIFIER
       ::= { ipfixSelectorMIB 2 }

   --==================================================================
   -- 1: Objects Used by All IPFIX Implementations
   --==================================================================
   --------------------------------------------------------------------
   -- 1.1: Packet Selector Functions for IPFIX
   --------------------------------------------------------------------
   ipfixSelectorFunctions OBJECT IDENTIFIER
       ::= { ipfixSelectorObjects 1 }

   --------------------------------------------------------------------
   -- 1.1.1: Function 1: Selecting All Packets
   --------------------------------------------------------------------
   ipfixFuncSelectAll OBJECT IDENTIFIER
       ::= { ipfixSelectorFunctions 1 }

   ipfixFuncSelectAllAvail OBJECT-TYPE
       SYNTAX      TruthValue
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "This object indicates the availability of the trivial
           function of selecting all packets.  This function is always
           available."
       ::= { ipfixFuncSelectAll 1 }






   --==================================================================
   -- 2: Conformance Information
   --==================================================================
   ipfixSelectorCompliances OBJECT IDENTIFIER
       ::= { ipfixSelectorConformance 1 }
   ipfixSelectorGroups      OBJECT IDENTIFIER
       ::= { ipfixSelectorConformance 2 }

   --------------------------------------------------------------------
   -- 2.1: Compliance Statements
   --------------------------------------------------------------------
   ipfixSelectorBasicCompliance MODULE-COMPLIANCE
       STATUS      current
       DESCRIPTION
           "An implementation that builds an IPFIX Exporter that
           complies with this module MUST implement the objects defined
           in the mandatory group ipfixBasicGroup.  The implementation
           of all other objects depends on the implementation of the
           corresponding functionality in the equipment."
       MODULE  -- this module
       MANDATORY-GROUPS {
               ipfixSelectorBasicGroup
       }
       ::= { ipfixSelectorCompliances 1 }

   --------------------------------------------------------------------
   -- 2.2: MIB Grouping
   --------------------------------------------------------------------
   ipfixSelectorBasicGroup OBJECT-GROUP
       OBJECTS {
           ipfixFuncSelectAllAvail
       }
       STATUS      current
       DESCRIPTION
           "The main IPFIX objects."
       ::= { ipfixSelectorGroups 1 }

   END














